##########################################################################################
##########################################################################################
# Lounge Mains Dimmer
# V1.0 2025-09-05 Fiest Attempt
##########################################################################################
# NOTES
# - 
# D5 = GPIO14  ZC
# D6 = GPIO12  PWM
#
##########################################################################################
##########################################################################################

##########################################################################################
# SPECIFIC DEVICE VARIABLE SUBSTITUTIONS
# If NOT using a secrets file, just replace these with the passwords etc (in quotes)
##########################################################################################
substitutions:
  # Device Naming 
  device_name: "esp-loungemainsdimmer1"
  friendly_name: "Lounge Lighting Mains Dimmer 1"
  description_comment: "tba"
  device_area: "Lounge" # Allows ESP device to be automatically linked to an 'Area' in Home Assistant.  

  # Project Naming
  project_name: "Generic ESP8266.D1 Mini" # Project Details 
  project_version: "v3.5"  # Project V denotes release of yaml file, allowing checking of deployed vs latest version

  # Passwords & Secrets
  api_key: !secret esp-api_key # unfortunately you can't use substitutions inside secrets names
  ota_pass: !secret esp-ota_pass # unfortunately you can't use substitutions inside secrets names
  static_ip_address: !secret esp-loungemainsdimmer1_ip
  #mqtt_local_command_main_topic: !secret mqtt_local_command_main_topic
  #mqtt_local_status_main_topic: !secret mqtt_local_status_main_topic

  # Device Settings
  #relay_icon: "mdi:lightbulb-group"
  log_level: "INFO" # Define logging level: NONE, ERROR, WARN, INFO, DEBUG (Default), VERBOSE, VERY_VERBOSE
  update_interval: "60s" # update time for for general sensors etc


#########################################################################################
# PACKAGES: Included Common Packages
# https://esphome.io/components/packages.html
##########################################################################################
packages:
  common_wifi: !include
    file: common/network_common.yaml
    vars:
      local_device_name: "${device_name}"
      local_static_ip_address: "${static_ip_address}"
      local_ota_pass: "${ota_pass}"
  common_api: !include
    file: common/api_common.yaml
    vars:
      local_api_key: "${api_key}"
  #common_webportal: !include
  #  file: common/webportal_common.yaml
  common_mqtt: !include
    file: common/mqtt_common.yaml
    vars:
      local_device_name: "${device_name}"
  #common_sntp: !include
  #  file: common/sntp_common.yaml
  common_general_sensors: !include
    file: common/sensors_common.yaml
    vars:
      local_friendly_name: "${friendly_name}"
      local_update_interval: "${update_interval}"

#########################################################################################
# ESPHome
# https://esphome.io/components/esphome.html
#########################################################################################
esphome:
  name: "${device_name}"
  friendly_name: "${friendly_name}"
  comment: "${description_comment}" # Appears on the esphome page in HA
  area: "${device_area}"
  project:
    name: "${project_name}"
    version: "${project_version}"
  #on_boot:       
  #  priority: 200
  #  then:
  #    - switch.turn_on: Relay_2

#########################################################################################
# ESP Platform and Framework
# https://esphome.io/components/esp32.html
#########################################################################################
esp8266:
  board: esp01_1m
  early_pin_init: False # Initialise pins early to known values. Recommended false where switches are involved. Defaults to True.
  board_flash_mode: dout # Default is dout

#########################################################################################    
# ESPHome Logging Enable
# https://esphome.io/components/logger.html
############################################# 
logger:
  level: "${log_level}"  #INFO Level suggested, or DEBUG for testing
  #baud_rate: 0 #set to 0 for no logging via UART, needed if you are using it for other serial things (eg PZEM)
  #esp8266_store_log_strings_in_flash: false
  #tx_buffer_size: 64

#########################################################################################
# STATUS LED
# https://esphome.io/components/status_led.html
#########################################################################################
status_led:
  pin:
    number: GPIO2
    inverted: yes

output:
  - platform: ac_dimmer
    id: dimmer1
    gate_pin: GPIO12
    zero_cross_pin:
      number: GPIO14
      mode: INPUT_PULLUP
      inverted: true
    method: leading
    init_with_half_cycle: false

light:
  - platform: monochromatic
    output: dimmer1
    name: Dimmable Light